Tender specification
————————————————————————————————————————
LED luminaire with prismatic cover (diffuser)
User interface: DALI bus
Control system: DALI-2
Mounting type: Insert
Mounting location: Ceiling
Dimensions: Length 595 mm x width 595 mm x height 35 mm
Installation dimensions: Installation length: 600 mm x installation width: 600 mm x installation depth: 110 mm
Weight: 2.14 kg
Protection rating: IP20
Protection class: II
Impact resistance: not specified
Permissible ambient temperature: -20 °C ... +40 °C
Color: black
Rated voltage: 220-240 V AC / 50-60 Hz
Inrush current: ≤ 15.3 A / 258 µs at 230 V AC
Power consumption: 36 W
Current consumption: < 0.3 A
Standby consumption: < 0.5 W
Control gear: BOKE BK-DWL040E-A1050ADP+connection box BK-BAS010
Diffuser: prismatic
Glare control: DDP (micro-prismatic)
Light emission: direct
Beam angle: 95 °
Unified Glare Rating (UGR): < 19
Luminous flux: 4500 lm
Luminous efficacy: > 120 lm/W
Color temperature: 4000 K
Dimmable: DALI dimmable
Color rendering index Ra: >80
Service life: ≥ 50,000 h (L80B50)
Conformity: CE, RoHS
Warranty: 5 years